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Description 
Plastic air ducts and fittings systems for supply and exhaust ventilation of premises. The system is quick, easy and clean, assembled without sealants or fixation, can be installed and used in any climate, reducing operating costs.
Made from plastic.
Sizes: rectangular 110x55, 220x55 and 220x90 mm, round Ø100, Ø125 and Ø150 mm.
Duct lengths from 500 to 1500 mm. 
Technical specifications
	System
	Extraction performance
	Temperature range

	110x55 / Ø100 mm
	Up to 250 m3/h
	        -5°C … +60°C

	220x55 / Ø125 mm
	Up to 600 m3/h
	        -5°C … +60°C

	220x90 / Ø150 mm
	Up to 900 m3/h
	        -5°C … +60°C
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Plastic air duct and fitting systems
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Pressure drop, straight duct
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